FIREWALL

enable

configure terminal

hostname CISCOFW-BERLIM04

interface g1/4

ip address 10.10.104.1 255.255.255.0

nameif inside

description REDE CLIENTES

exit

interface g1/2

ip address 172.30.104.1 255.255.255.0

nameif outisde

description REDE ROUTER-FIREWALL

exit

interface g1/3

ip address 172.31.104.1 255.255.255.0

nameif dmz

security-level 50

description REDE SERVIDORES

exit

access-list T1 extended permit icmp any any

access-group T1 in interface dmz